|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Hand and Power Tool Self Assessment** | | | | | |
| Makergrounds Location: |  | | | | |
| Inspection Completed By: |  | | | | |
| Inspection Date: |  | |  | |  |
| **Hand Tools** | **OK** | **Not OK** | **N/A** | **Corrective Action** | **Date Corrected** |
| Outside of tools are free of grease, oil, lubricant, and any other accumulated foreign matter? |  |  |  |  |  |
| Handles are free of cracks, breaks, splinters, sharp edges, and makeshift repairs? |  |  |  |  |  |
| Tips of screwdrivers, chisels or other similar tools show no excessive wear? |  |  |  |  |  |
| Gripping surfaces on pliers, wrenches or other similar tools are not worn, bent or show visible deformity? |  |  |  |  |  |
| Impact tools such as chisels and punches are free of mushroom heads? |  |  |  |  |  |
| Hammer heads are secure in handle, free from chips and show no visible damage? |  |  |  |  |  |
| Tools are not being hoisted or carried by their cords? |  |  |  |  |  |
| **Power Tools** | **OK** | **Not OK** | **N/A** | **Corrective Action** | **Date Corrected** |
| Power tools are properly grounded or double insulated to protect from shock hazard? |  |  |  |  |  |
| Power source shows no damage (frayed cord, visible damage on cord or plug end, charger in good condition, etc.) |  |  |  |  |  |
| Guards are in place and functional on power tools? |  |  |  |  |  |
| Blades or bits are not damaged, cracked or excessively worn? |  |  |  |  |  |
| Compressed air under 30psi when used for cleaning? |  |  |  |  |  |
| Comments: | | | | | |