|  |
| --- |
| **Hand and Power Tool Self Assessment** |
| Makergrounds Location: |   |
| Inspection Completed By: |   |
| Inspection Date: |   |   |   |
| **Hand Tools** | **OK** | **Not OK** | **N/A** | **Corrective Action** | **Date Corrected** |
| Outside of tools are free of grease, oil, lubricant, and any other accumulated foreign matter? |   |   |   |   |   |
| Handles are free of cracks, breaks, splinters, sharp edges, and makeshift repairs? |   |   |   |   |   |
| Tips of screwdrivers, chisels or other similar tools show no excessive wear? |   |   |   |   |   |
| Gripping surfaces on pliers, wrenches or other similar tools are not worn, bent or show visible deformity? |   |   |   |   |   |
| Impact tools such as chisels and punches are free of mushroom heads? |   |   |   |   |   |
| Hammer heads are secure in handle, free from chips and show no visible damage? |   |   |   |   |   |
| Tools are not being hoisted or carried by their cords? |   |   |   |   |   |
| **Power Tools** | **OK** | **Not OK** | **N/A** | **Corrective Action** | **Date Corrected** |
| Power tools are properly grounded or double insulated to protect from shock hazard? |   |   |   |   |   |
| Power source shows no damage (frayed cord, visible damage on cord or plug end, charger in good condition, etc.) |   |   |   |   |   |
| Guards are in place and functional on power tools? |   |   |   |   |   |
| Blades or bits are not damaged, cracked or excessively worn? |   |   |   |   |   |
| Compressed air under 30psi when used for cleaning?  |   |   |   |   |   |
| Comments: |