|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Electrical Cord Self- Assessment** | | | | | |
| Makergrounds Location: |  | | | | |
| Inspection Completed By: |  | | | | |
| Inspection Date: |  | | # Cords Inspected: | |  |
| **Electrical Cord Inspection** | **OK** | **Not OK** | **N/A** | **Corrective Action** | **Date Corrected** |
| Extension cords are used for temporary purposes and not as a replacement for fixed / permanent wiring? |  |  |  |  |  |
| Daisy chaining extension cords/power strips prohibited? |  |  |  |  |  |
| Extension cords not run through doorways, windows, unprotected openings or holes in walls? |  |  |  |  |  |
| Power and Extension cords are run so that they do not create tripping hazards? |  |  |  |  |  |
| All cords are in good repair with no damage to outer jacket insulation (damage/fraying), plugs or pins? |  |  |  |  |  |
| All power cords are grounded cords, with the grounding pin intact? Cheater plugs (adapters) are not being used? |  |  |  |  |  |
| All damaged extension cords and equipment with damaged cords have been removed from service? |  |  |  |  |  |
| Tools are not being hoisted or carried by their cords? |  |  |  |  |  |
| Comments: | | | | | |