|  |
| --- |
| **Electrical Cord Self- Assessment** |
| Makergrounds Location: |   |
| Inspection Completed By: |   |
| Inspection Date: |   | # Cords Inspected: |   |
| **Electrical Cord Inspection** | **OK** | **Not OK** | **N/A** | **Corrective Action** | **Date Corrected** |
| Extension cords are used for temporary purposes and not as a replacement for fixed / permanent wiring?  |   |   |   |   |   |
| Daisy chaining extension cords/power strips prohibited?  |   |   |   |   |   |
| Extension cords not run through doorways, windows, unprotected openings or holes in walls?  |   |   |   |   |   |
| Power and Extension cords are run so that they do not create tripping hazards? |   |   |   |   |   |
| All cords are in good repair with no damage to outer jacket insulation (damage/fraying), plugs or pins?  |   |   |   |   |   |
| All power cords are grounded cords, with the grounding pin intact? Cheater plugs (adapters) are not being used? |   |   |   |   |   |
| All damaged extension cords and equipment with damaged cords have been removed from service? |   |   |   |   |   |
| Tools are not being hoisted or carried by their cords? |   |   |   |   |   |
| Comments: |